**Volkslogger Setup and Use**

Open “See You”

 At “confirm” prompt select **yes**

Go to “Tools” “Pilots”

 Enter pilot data, then “Add” tab

Open “Task” icon

 Position and Zoom map as desired

 On bottom left corner of screen shows W A V R

 W = Way Point

 A = Air Space

 V = Vector (topology)

 R = Raster

 Click on parameters desired

 At “Tools” “Airspace” change colors, etc. as desired

**To add a task:**

L click on “Add Task” icon

L click on Triangle + icon

L click on Meadow Lake or starting point

Move cursor to 1st destination L click

Move cursor to next destination and L click

Repeat above 2 steps as desired

Double click on final destination and the **Esc**

 See You now has task setup and defined.

**To set up logger:**

Select “File”, then select “Connection Wizard”

Verify that screen shows “Volkslogger” “Auto” “Auto”

Plug in 3 connector cable to PC, battery & logger

PC should show “connected to S/N 2KG”

From PC screen, check “Upload flight declaration to device”

“Next”

Go to “People” icon & L click

 Double click on desired pilot

 Change plane data, etc. as needed

Double click on double triangle icon

 Double click on the desired task, then “Next” if desired task appears

 Upload flight declaration. Logger shows “receiving data”

 Wait for “Upload Complete”

 Select “Finish”

Unplug logger and then plug it back in

Install in plane and connect to battery

Verify satellite lock

Go fly

Let run for a few minutes after flight

**Volkslogger general button purpose:**

 Top button cycles between screens

 Middle button cycles through way points in flight

Bottom button acts as a select button on menu screens

**After Flight:**

Start See You

Plug logger into PC

 Select “Download flights from device”

“Next”

Logger says “Data transfer Ready”

Verify “Open flight after download” and “Secure Mode” are selected

“Next”

Screen should show “data transfer calculating key”

Wait for transfer to complete

**To Clear the Volkslogger Memory:**

Toggle top button until “ACT” shows

Toggle middle button to select “ACT”

Click bottom button to select “ACT”

Toggle middle button to “Mem Clr”

Click bottom button to select “Mem Clr”

Middle button to “yes”

Bottom button to select “yes”